**Aeris MIRA HCHO Analyzer Data Flag Key**

No flag = is a valid sample

ND = Non-detect (defined as a true non-detect, or reported value less than 0.001 ppb and greater than negative of the MDL)

MD = Detected, but less than the method detection limit (MDL)

II = Instrument Issue, data is invalidated. No value reported, and should not be included in statistical analysis.

BG = Instrument measuring formaldehyde-scrubbed air to determine background, no value reported to prevent being included in statistical analysis.

Cal = Instrument performing a calibration during this time, no value reported to prevent being included in statistical analysis.