**Pyxis VOC Data Flag Key**

No flag = is a valid sample

ND = Non-detect (defined as a true non-detect, or reported value less than 0.001 ppb). Defined as zero for statistical purposes.

MD = Detected, but less than the method detection limit (MDL). Defined as half MDL for statistical purposes.

II = Instrument Issue, data is invalidated. No value reported, and should not be included in statistical analysis.